**For Video Streaming using Raspberry Pi**

1. Click on Raspberry Button, Click on Preferences, Click on RaspberryPi Configuration and Enable all
2. Run the following command - raspivid -o - -t 0 -w 800 -h 600 -fps 12 | cvlc -vvv stream:///dev/stdin --sout '#rtp{sdp=rtsp://:8080/}' :demux=h264
3. Open VLC Media Player, Click on Media. Open Network Stream or Click Ctrl+N
4. Paste the command - rtsp://raspberrypi:8080/

Put the camera in front of the face.

**Note : If you get the error of Imutils Library. Please run the following commands-**

1. sudo pip3 uninstall imutils
2. sudo pip3 install --upgrade imutils